#
PLASTIC PARTS HEAT RESISTING TEMPERATURE

BME098050000701

Part Name | Code | Material Name | Heat resisting Temperature°C{°F}
--- | --- | --- | ---
FRONT WINDOW UPPER MOLDING | PVC | POLYVINYLCHLORIDE | 95 {203}
COWL GRILLE | PP | POLYPROPYLENE | 110 {230}
HEAD LIGHT | LENS | PC | POLYCARBONATE | 130 {266}
HOUSING | PP | POLYPROPYLENE | 120 {248}
FRONT BUMPER | PP | POLYPROPYLENE | 100 {212}
RADIATOR GRILLE | ABS | ABS | 70 {158}
FRONT COMBINATION LIGHT | LENS | PMMA | ACRYLIC | 75 {167}
HOUSING | ABS | ABS (HEAT RESISTING SPECS.) | 70 {158}
FRONT SIDE TURN LIGHT | LENS | PMMA | ACRYLIC | 75 {167}
HOUSING | ABS | ABS (HEAT RESISTING SPECS.) | 70 {158}
OUTER HANDLE | PC | POLYCARBONATE | 130 {266}
ROOF MOLDING | PET-PBT | POLYETHYLENETEREPHTHALATE-PBT | 60 {140}
OUTSIDE MIRROR | AAS | AAS | 80 {176}
OUTSIDE MIRROR | BLACK | AAS | AAS | 80 {176}
BODY COLOR | ABS | ABS | 80 {176}
SIDE PROTECTOR | PVC | POLYVINYLCHLORIDE | 50 {122}
RAIL PROTECTOR | PC-PET | POLYCARBONATE-POLYETHYLENETEREPHTHALATE | 120 {248}
REAR BUMPER | PP | POLYPROPYLENE | 100 {212}
REAR COMBINATION LIGHT | LENS | PMMA | ACRYLIC | 75 {167}
HOUSING | PC-PET | POLYCARBONATE-POLYETHYLENETEREPHTHALATE | 120 {248}
LIFTGATE GARNISH | ABS | ABS | 70 {158}
REAR WINDOW MOLDING | PVC | POLYVINYLCHLORIDE | 95 {203}
HIGH-MOUNT BRAKE LIGHT | LENS | PC | POLYCARBONATE | 130 {266}
HOUSING | PC | POLYCARBONATE | 130 {266}

  Note

  • The application of temperatures higher than heat resisting temperatures may result in part deformation.