#
CONTROL SYSTEM BLOCK DIAGRAM [AJ]

BME014000000T56

1 | MAF sensor
2 | IAT sensor (in MAF sensor)
3 | CKP sensor
4 | CMP sensor
5 | ECT sensor
6 | HO2S
7 | TP sensor
8 | Knock sensor
9 | BARO sensor (European (L.H.D.) specs.)/EGR boost sensor (Australian, General (L.H.D. R.H.D.) specs.)
10 | TR switch
11 | PSP switch
12 | VSS
13 | Immobilizer unit
14 | A/C switch
15 | Brake switch
16 | Generator (terminal P)
17 | DLC (terminal TEN)
18 | Battery
19 | PCM
20 | Idle air control (IAC)
21 | Fuel injection control
22 | Electronic spark advance (ESA) control
23 | Fuel pump control
24 | Front HO2S heater control
25 | Rear HO2S heater control (European (L.H.D.) specs.)
26 | Electrical fan control
27 | Purge control
28 | EGR control
29 | Intake manifold communication control (IMCC)
30 | A/C cut-off control
31 | Generator control
32 | ECT output function
33 | Immobilizer system
34 | IAC valve
35 | Fuel injector
36 | Ignition coil
37 | Fuel pump relay
38 | Front HO2S heater
39 | Rear HO2S heater (European (L.H.D.) specs.)
40 | Fan control module
41 | Purge solenoid valve
42 | EGR valve
43 | IMCC actuator
44 | A/C relay
45 | Generator (terminal D)
46 | Water temperature gauge