#
CLUTCH

BME055001024201

Item | Specification
--- | ---
Manual transaxle type | G15M-R | A65M-R
Clutch pedal | Height (with carpet) | mm {in} | 231-236 {9.09-9.29} (Reference value)
Free play | Pedal free play | mm {in} | 5.2-14 {0.20-0.55}
Push rod free play at clutch pedal | mm {in} | 0.1-0.5 {0.004-0.02} (Reference value)
Disengagement point | Disengagement stroke | mm {in} | 23-43 {0.91-1.69}
Pedal stroke | mm {in} | 148 {5.83} (Reference value)
Clutch cover | Diaphragm spring fingers | Maximum depth | mm {in} | 0.6 {0.024}
Maximum height difference | mm {in} | 0.6 {0.024}
Maximum clearance of flatness of the pressure plate | mm {in} | 0.3 {0.012}
Clutch disc | Minimum depth | mm {in} | 0.3 {0.012}
Maximum runout | mm {in} | 0.7 {0.028}
Flywheel | Maximum runout | mm {in} | 0.1 {0.004} | 0.3 {0.012}