#
NO.2 VEHICLE MOVES IN N POSITION [JA5A-EL]

BME050301030238

2 | Vehicle moves in N position
DESCRIPTION | • Vehicle creeps in N position. • Vehicle creeps if brake pedal is not depressed in N position.
POSSIBLE CAUSE | • If the vehicle moves in N position, basically, the malfunction is in ATX. Since a malfunction is in the sensor circuit or output circuit is the cause of the malfunction in the ATX, inspect the sensors, output circuit, and the related harnesses.

  1. Clutch burnt (Low clutch, Low one-way clutch, Low and reverse brake)

  • Line pressure low
  • Control valve body malfunction

  2. Selector lever position disparity (Although the selector indicator shows N position, the hydraulic circuit shows D range or R position)

  Note

  • Before following the troubleshooting steps, make sure that the Automatic Transaxle On-Board Diagnostic and Automatic Transaxle Basic Inspection are conducted.

Diagnostic procedure

STEP | INSPECTION | ACTION
--- | --- | ---
1 | Does the vehicle creep when the selector lever is moved slightly in N position? | Yes | Overhaul the control valve body and repair or replace any malfunctioning parts. (See ATX Workshop Manual.) If any problem remains, replace or overhaul the transaxle and repair or replace any malfunctioning parts. (See AUTOMATIC TRANSAXLE REMOVAL/INSTALLATION [JA5A-EL].)
(See ATX Workshop Manual.)
No | Inspect and adjust selector lever. (See SELECTOR LEVER INSPECTION.) (See SELECTOR CABLE ADJUSTMENT.)
2 | • Verify the test results.

  - If normal, return to the diagnostic index to service any additional symptoms.
  - If the malfunction remains, inspect the related Service Bulletins and/or On-line Repair Information and perform repair or diagnosis.

  • If the vehicle is repaired, troubleshooting is completed.
  • If the vehicle is not repaired or additional diagnostic information is not available, replace the TCM.