#
CLUTCH PEDAL REMOVAL/INSTALLATION

BME051041030W04

1. Remove the air cleaner. (L.H.D. models)

2. Remove the battery. (L.H.D. models)

3. Remove in the order indicated in the table.

4. Install in the reverse order of removal.

5. After installation, adjust the clutch pedal. (See CLUTCH PEDAL INSPECTION/ADJUSTMENT.)

1 | Nut
2 | Clutch switch connector
3 | Clutch switch
4 | Nut
5 | E-clip
6 | Pin
7 | Bushing
8 | Nut
9 | Push rod
10 | Clevis
11 | Pedal pad
12 | Clutch pedal (See Clutch Pedal Installation Note.)

## Clutch Pedal Installation Note

1. After installation, adjust the pedal height and free play. (See CLUTCH PEDAL INSPECTION/ADJUSTMENT.)