#
SIDE PROTECTOR INSTALLATION

BME091650680202

1. Remove the adhesive remaining on the side protector (if it will be reused) and the body using a razor.

2. Remove any grease or dirt from the adhesion surface of the side protector (if it will be reused) and the body.

3. Attach double-sided adhesive tape to the side protector as shown (if it will be reused).

Clearance

  a: 7.0-9.0 mm {0.28-0.35 in}
  b: 34.0-36.0 mm {1.39-1.42 in}
  c: 37.0-39.0 mm {1.46-1.54 in}
  d: 1.0-3.0 mm {0.04-0.11 in}
  e: 0.0-2.0 mm {0.00-0.08 in}
  f: 6.0 mm {0.24 in}
  g: 1.0-3.0 mm {0.04-0.11 in}

4. Peel off the backing paper from the double-sided adhesive tape and attach the side protector onto the body as shown.

Clearance

  a: 1.0-4.0 mm {0.04-0.15 in}
  b: 1.0-4.0 mm {0.04-0.15 in}
  c: 100 mm {3.94 in}
  d: 200 mm {7.84 in}
  e: 284.1 mm {11.19 in}
  f: 308.1 mm {12.13 in}