#
BLOWER UNIT CONSTRUCTION

BME071161140T01

## Air intake

• The blower unit has two air inlets for recirculating to increase the speed of interior air circulation. This enables rapid cooling of air (recirculating).

## Air filter

• The air filter removes pollen and dust from the air to supply fresh air to the passenger compartment.
• The air filter is installed over the blower fan, and absorbs the air-intake noise and motor operating noise.

  Note

  • Because the air filter cannot be cleaned or reused, it must be replaces periodically.

Replace the air filter

  • ISRAEL specs.: Once a year or every 15,000 km {9,000 miles}.
  • General (L.H.D. R.H.D.) specs.: Once a year or every 20,000 km {12,000 miles}.
  • European (L.H.D. U.K.) specs.: Once every two years or every 40,000 km {25,000 miles}.

1 | Air intake door
2 | Air filter
3 | Recirculate
4 | Fresh
5 | To front A/C unit