#
WATER PUMP REMOVAL/INSTALLATION [MZR-CD (RF Turbo)]

BME011215010W03

1. Disconnect the negative battery cable.

2. Drain the engine coolant. (See COOLING SYSTEM SERVICE WARNINGS.)(See ENGINE COOLANT REPLACEMENT [MZR-CD (RF Turbo)].)

3. Remove the timing belt. (See TIMING BELT REMOVAL/INSTALLATION [MZR-CD (RF Turbo)].)

4. Remove in the order indicated in the table.

5. Install in the reverse order of removal.

6. Refill the engine coolant. (See ENGINE COOLANT REPLACEMENT [MZR-CD (RF Turbo)].)

1 | Hose
2 | Lower radiator hose
3 | Thermostat case
4 | Water pump