#
RADIATOR REMOVAL/INSTALLATION [MZR-CD (RF Turbo)]

BME011215200W03

1. Disconnect the negative battery cable.

2. Drain the engine coolant. (See COOLING SYSTEM SERVICE WARNINGS.)(See ENGINE COOLANT REPLACEMENT [MZR-CD (RF Turbo)].)

3. Remove the front bumper. (See FRONT BUMPER REMOVAL/INSTALLATION.)

4. Remove the hood lock release lever.

5. Remove in the order indicated in the table.

6. Install in the reverse order of removal.

7. Refill the engine coolant. (See ENGINE COOLANT REPLACEMENT [MZR-CD (RF Turbo)].)

1 | Fan control module connectors
2 | Fan control module (See COOLING FAN MOTOR REMOVAL/INSTALLATION [MZR-CD (RF Turbo)].)
3 | Resevoir hose
4 | Radiator hose
5 | Radiator bracket
6 | Air seal
7 | Radiator (See Radiator Removal/Installation Note.)

## Radiator Removal/Installation Note

1. Pull the fan component backward to obtain the clearance, and remove/install the radiator.