#
DIFFERENTIAL ASSEMBLY

BME051527100303

## Assembly Procedure

1. Apply specified oil to each part immediately before assembly.

2. Set the speedometer drive gear onto the gear case.

3. Install the bearing using the SST.

4. Install the thrust washer to the gear case.

5. Install the side gear.

6. Install the pinion gears and thrust washers into the gear case.

7. Install the pinion carrier.

8. Install the pinion shafts.

  Caution

  • Assemble the roll pin so that the roll pin opening is perpendicular to the pinion shaft.

9. Install the roll pin, and crimp it to prevent it from coming out of the gear case.

10. Install the side gear and thrust washer.

11. Install the differential cover.

  Tightening torque
  7.8-10.8 N·m {80-110 kgf·cm, 69.5-95.4 in·lbf}

12. Measure the backlash of the side gear as follows:

  (1) Install the left and right drive shafts in the differential.
  (2) Support the drive shaft on V-blocks.
  (3) Measure the backlash of both side gears.

  • If not within the specification, reassemble the differential.

  Backlash
  Standard: 0.025-0.10 mm {0.0010-0.0039 in}
  Maximum: 0.10 mm {0.0039 in}

13. Install the ring gear.

14. Tighten the bolts evenly and gradually in the order as shown in the figure.

  Tightening torque
  152-176.5 N·m {15.5-17.9 kgf·m, 112-130 ft·lbf}