#
POWER WINDOW SYSTEM OUTLINE

BME091258000T03
• The driver-side power window system, which has an auto-close and auto-open functions with an automatic window return function, is the same as that of the current PREMACY (CP) model. (Australian, European (L.H.D. U.K.), General (R.H.D.) specs.)
• The power window system is the same as that of the current 626 (GF) model. (General (L.H.D.) Specs.)
• IG OFF timer function has been adopted. The function is the same as that of the current 121/121 DEMIO (DW) model. (See Mazda 121/121 DEMIO Workshop Manual Supplement 1675-1*-00A.)
• Two-step down function has been adopted for the driver-side power window system. The function is the same as that of the current PREMACY (CP) model. (See Mazda PREMACY Workshop Manual Supplement 1718-1*-01G.)
× : Applied

Function | European (L.H.D.) specs. | U.K. specs. | Australian specs. | General (L.H.D.) specs. | General (R.H.D.) specs.
--- | --- | --- | --- | --- | ---
Manual open | × | × | × | × | ×
Manual close | × | × | × | × | ×
Auto open | × | × | × | × | ×
Auto close | × | × | × | N/A | ×
Power-cut | × | × | × | × | ×
Automatic window return function | × | × | × | N/A | ×
IG OFF timer function | × | × | × | × | ×
Two-step down function | × | × | × | × | ×