#
SIDE PROTECTOR INSTALLATION

BME091650680W02

1. Remove the adhesive remaining on the side protector (if it will be reused) and the body using a razor.

2. Remove any grease or dirt from the adhesion surface of the side protector (if it will be reused) and the body.

3. Attach double-sided adhesive tape to the side protector as shown (if it will be reused).

Clearance

  a: 4.0-6.0 mm {0.16-0.23 in}
  b: 29.0-31.0 mm {1.15-1.22 in}
  c: 1.0-3.0 mm {0.04-0.11 in}
  d: 6.0-8.0 mm {0.24-0.31 in}
  e: 44.0-46.0 mm {1.74-1.81 in}
  f: 10.0 mm {0.39 in}

4. Peel off the backing paper from the double-sided adhesive tape and attach the side protector onto the body as shown.

Clearance

  a: 1.0-4.0 mm {0.04-0.15 in}
  b: 1.0-4.0 mm {0.04-0.15 in}
  c: 100 mm {3.94 in}
  d: 200 mm {7.84 in}
  e: 251.5-254.5 mm {9.91-10.01 in}
  f: 266.5-269.5 mm {10.50-10.61 in}