#
SELECTOR CABLE ADJUSTMENT

BME051846102202

1. Remove the column cover.

2. Shift the selector lever to P position.

3. Loosen nut A as shown in the figure.

4. Pull the selector lever to the R position side gate of P position, and tighten nut A.

Tightening torque

  15.7-22.5 N·m {1.6-2.2 kgf·m, 11.6-16.5 ft·lbf}

5. Verify that the selector lever bolt end is exposed from the nut.

6. Install the column cover.