#
FUEL TANK REMOVAL/INSTALLATION [L3]

BME011442110201

  Warning

  • Repairing a fuel tank that has not been properly steam cleaned can be dangerous. Explosion or fire may cause death or serious injury. Always properly steam clean a fuel tank before repairing it.
  • Fuel line spills and leakage are dangerous. Fuel can ignite and cause serious injuries or death and damage. Fuel can also irritate skin and eyes. To prevent this, do not damage the sealing surface of the fuel pump unit when removing or installing.

  Caution

  • Disconnecting/connecting the quick release connector without cleaning it may possibly cause damage to the fuel pipe and quick release connector. Always clean the quick release connector joint area before disconnecting/connecting using a cloth or soft brush, and make sure that it is free of foreign material.

1. Level the vehicle.

2. Complete the "BEFORE SERVICE PRECAUTION". (See BEFORE SERVICE PRECAUTION [L3].)

3. Disconnect the negative battery cable.

4. Remove the fuel pump unit. (See FUEL PUMP UNIT REMOVAL/INSTALLATION [L3].)

5. Siphon the fuel from the fuel tank.

6. Remove in the order indicated in the table.

7. Install in the reverse order of removal.

8. Complete the "AFTER SERVICE PRECAUTION". (See AFTER SERVICE PRECAUTION [L3].)

1 | Joint hose (See Joint Hose Installation Note)
2 | Breather hose (See Breather Hose Installation Note)
3 | Evaporative hose (See Evaporative Hose Installation Note)
4 | Fuel tank
5 | Fuel-filler pipe protector
6 | Fuel-filler pipe
7 | Nonreturn valve

## Evaporative Hose Installation Note

1. Fit evaporative hose onto the respective fittings, and install clamps as shown.

## Breather Hose Installation Note

1. Fit the breather hose onto the respective fittings, and install clamps as shown.

## Joint Hose Installation Note

1. Fit the joint hose onto the respective fittings, and install clamps as shown.