#
GLASS ANTENNA INSPECTION

BME092066931W01

## AM Radio Antenna

1. Inspect the glass antenna for damage visually.

2. Inspect for continuity between the glass antenna terminals using an ohmmeter.

  • If not as specified, replace the glass antenna. (See FILAMENT REPAIR.)

## FM Radio Antenna

1. Inspect the glass antenna for damage visually.

2. Inspect for continuity between the glass antenna terminals using an ohmmeter.

  • If not as specified, repair the glass antenna. (See FILAMENT REPAIR.)