#
AFTER REPAIR PROCEDURE [MZR-CD (RF Turbo)]

BME011400000W07

  Warning

  • Fuel line spills and leakage are dangerous. Fuel can ignite and cause serious injuries or death and damage. When installing the fuel hose, observe "Fuel Hose Installation" described below.

  Caution

  • If fuel does not pass through the fuel filter, foreign material may have penetrated in the supply pump, and this may cause a malfunction resulting in damage to the supply pump. Therefore, do not install the fuel hoses (main and return side) in reverse. When installing the fuel hose, always follow the Fuel Hose Installation Note in the Workshop Manual and perform the procedure. (See Fuel Hose Installation Note.)

## Fuel Line Air Bleeding

  Caution

  • Continuously cranking the engine for over 30 seconds can damage the battery and the starter.

1. Continue cranking the engine for 30 seconds and stop for 5-10 seconds until the engine starts.

## Fuel Hose Installation

1. Verify that there is no damage or deformation on the fuel hose and fuel pipe when installing.

2. When installing the fuel hose connected to the supply pump, verify each side (main and return), and install at the specified position. (See Fuel Hose Installation Note.)