#
VALVE, VALVE SPRING, VALVE SEAL GUIDE CONSTRUCTION [AJ]

BME011012111T03
• Heat-resistant steel rods have been adopted on the four valves, with two intake valves and two exhaust valves per cylinder.
• A valve seal integrated into the lower valve spring seat has been adopted for simplification and improved serviceability.

1 | Valve keeper
2 | Upper valve spring seat
3 | Valve spring
4 | Valve seal
5 | Valve guide
6 | Valve