#
CALIPER (REAR) DISASSEMBLY/ASSEMBLY

BME041126990201

1. Disassemble in the order indicated in the table.

1 | Dust seal
2 | Piston (See Piston Disassembly Note)
3 | Piston seal (See Piston Seal Disassembly Note)
4 | Bleeder cap
5 | Bleeder screw
6 | Caliper

2. Assemble in the reverse order of removal.

## Piston Disassembly Note

  Caution

  • Blow the compressed air slowly to prevent the piston from suddenly popping out.

1. Place a piece of wood in the caliper, then blow compressed air through the hole to force the piston out of the caliper.

## Piston Seal Disassembly Note

1. Remove the piston seal from the brake caliper using the SST.