#
SAS UNIT REMOVAL/INSTALLATION

BME081057030W01

  Warning

  • Handling the SAS unit improperly can accidentally deploy the air bag modules, which may seriously injure you. Read AIR BAG SYSTEM SERVICE WARNINGS before handling the SAS unit. (See SERVICE WARNINGS.)

1. Turn the ignition switch to LOCK position.

2. Disconnect the negative battery cable and wait for more than 1 minute.

3. Partially peel off the floor covering.

4. Remove in the order indicated in the table.

5. Install in the reverse order of removal.

6. Turn the ignition switch to ON position.

7. Verify that the air bag system warning light illuminates for approximately 6 seconds and then goes off.

  • If the air bag system warning light does not operate in the manner described above, there are malfunctions in the system. Inspect the system using the on-board diagnostic.

  Note

  • When a new SAS unit has been installed, the air bag system warning light flashes continuously if there are no malfunctions in the system. Perform the air bag module and pre-tensioner seat belt deployment authorization procedure. (See AIR BAG MODULE AND PRE-TENSIONER SEAT BELT DEPLOYMENT AUTHORIZATION PROCEDURES.)

1 | Connector
2 | Nut
3 | SAS unit