#
REAR PILLAR (INNER) INSTALLATION

BME098070120B04

1. Welding of (A) should be performed during installation of the rear fender panel.

2. Drill holes for plug welds before installing new parts.

3. When joining the new and old parts, temporarily install and fit the new part in position, measure each dimension according to the body dimension drawing, then adjust the position to align it to the standard dimension.