#
HOLD INDICATOR LIGHT INSPECTION [JA5A-EL]

BME051755480201

## Operation Inspection

1. Turn the ignition switch to the ON position.

  Note

  • The HOLD indicator light will illuminate if a malfunction exists in any of the EC-AT system components.

2. Verify that the HOLD indicator light is not illuminated.

3. Press the switch and verify that the HOLD indicator illuminates.

  • If there is any malfunction, after checking the HOLD switch (See HOLD SWITCH INSPECTION [JA5A-EL].), inspect the terminal voltage of the HOLD indicator light.

## Voltage Inspection

1. Turn the ignition switch to the ON position.

2. Measure voltage between terminal 3J and a ground.

Voltage | Action
--- | ---
B+ | Go to the next step
Other | • Replace METER fuse • Repair the wiring harness (METER fuse-instrument cluster)

## Continuity Inspection

1. Disconnect the instrument cluster connector.

2. Disconnect the TCM connector.

3. Inspect continuity between instrument cluster connector terminal 1H and TCM terminal 1E.

  • If there is any malfunction, inspect the wiring harness (instrument cluster-TCM).
  • If if is normal, go to the next step.

Terminals | Continuity
--- | ---
1H- (TCM 1E) | Yes

4. Inspect continuity between terminals 1H and 3J.

  • If there is any malfunction, replace the instrument cluster or bulb.

Terminals | Continuity
--- | ---
1H-3J | Yes