#
DRIVE BELT INSPECTION [MZR-CD (RF Turbo)]

BME011015800205

  Note

  • Front and water pump drive belt deflection/tension inspection is not necessary because of the use of the front drive belt auto tensioner.

## Front Drive Belt

1. Verify that the drive belt auto tensioner indicator mark does not exceeds the limit.

  • If it exceeds the limit, replace the drive belt. (See DRIVE BELT REPLACEMENT [MZR-CD (RF Turbo)].)