#
ACCELERATOR CABLE ADJUSTMENT [AJ]

BME011341660204

1. Move the white locking tab A to the unlock position.

2. Turn stopper B to the unlock position.

  Note

  • If stopper B will not unlock, it may be necessary to carefully bend tab C out using a suitable tool.

3. To adjust the free play, push or pull the throttle cable housing directly behind the spring.

4. Measure the throttle cable free play, making sure that it is within the specification.

Free play

  1.5-4.0 mm {0.06-0.15 in}

5. Turn stopper B to lock position.

6. Move the white locking tab A to the lock position.

7. Verify correct accelerator operation.