#
REAR SHOCK ABSORBER AND SPRING REMOVAL/INSTALLATION

BME021405910201

  Caution

  • Performing the following procedures without first removing the ABS wheel-speed sensor may possibly cause an open circuit in the harness if it is pulled by mistake. Before performing the following procedures, remove the ABS wheel-speed sensor (axle side) and fix it to an appropriate place where the sensor will not be pulled by mistake while servicing the vehicle.
  • Be careful when using the jack to avoid damaging the brake pipe and hose.

1. Remove in the order indicated in the table.

2. Install in the reverse order of removal.

1 | Brake caliper component (See Brake Caliper Removal Note.)
2 | ABS sensor harness bracket (with ABS)
3 | Rear shock absorber (See Rear Shock Absorber Removal Note.)
4 | Coil spring
5 | Upper spring seat rubber
6 | Lower spring seat rubber
7 | Bound stopper

## Rear Shock Absorber Removal Note

1. Support the lower torsion beam axle using a jack, and jack up the torsion beam axle until the shook absorber is free.

2. Remove the shock absorber.