#
SUNROOF MOTOR INSPECTION

BME091569870W02

## Motor

1. Remove the sunroof motor.

2. Apply battery positive voltage to the sunroof motor terminals and inspect the operation of the sunroof motor.

  • If not as specified, replace the sunroof motor.

Connection | Motor operation
--- | ---
2K | 2M
B+ | GND | Turn right (Open/Tilted down)
GND | B+ | Turn left (Closed/Tilted up)

## Limit Switch

1. Remove the headliner.

2. Verify the glass panel position.

3. Disconnect the connector.

4. Inspect for continuity between the sunroof motor terminals using an ohmmeter.

  • If not as specified, replace the sunroof motor.