#
PARKING LIGHT BULB REMOVAL/INSTALLATION

BME091851040201

1. Disconnect the negative battery cable.

2. Remove in the order indicated in the table.

1 | Socket (See Socket Removal Note (Left Side Only))
2 | Parking light bulb
3 | Connector

3. Install in the reverse order of removal.

## Socket Removal Note (Left Side Only)

1. Remove the battery.

2. Remove the fresh-air duct installation bolt.

3. Slide the fresh-air duct to the right, and ensure space for the socket removal.