#
PRIMARY SHAFT END PLAY ADJUSTMENT

BME051501029M02

  Note

  • Adjust the primary shaft end play by measuring the clearance between the transaxle case and the primary shaft rear bearing, and selecting a primary shaft bearing adjustment shim.
  • Calculate adjustment shim thickness O as defined below to adjust the primary shaft bearing end play to standard.

  Standard: 0.00-0.06 mm {0.0000-0.0024 in}
  Dimension O = (O1 - O2) - end play
  O: adjustment shim thickness
  O1: transaxle case contact face and adjustment shim installation surface dimension
  O2: clutch housing contact face and primary shaft rear bearing contact face dimension

Adjustment shim thickness

(mm {in})

0.40 {0.016} | 0.76 {0.030} | 1.12 {0.044} | 1.48 {0.058}
0.44 {0.017} | 0.80 {0.031} | 1.16 {0.046} | 1.52 {0.060}
0.48 {0.019} | 0.84 {0.033} | 1.20 {0.047} | 1.56 {0.061}
0.52 {0.020} | 0.88 {0.035} | 1.24 {0.049} | 1.60 {0.063}
0.56 {0.022} | 0.92 {0.036} | 1.28 {0.050} | 1.64 {0.065}
0.60 {0.024} | 0.96 {0.038} | 1.32 {0.052} | 1.68 {0.066}
0.64 {0.025} | 1.00 {0.039} | 1.36 {0.054} | 1.72 {0.068}
0.68 {0.027} | 1.04 {0.041} | 1.40 {0.055} | -
0.72 {0.028} | 1.08 {0.043} | 1.44 {0.057} | -

1. Measure dimension O1 for the clutch housing installation surface of the transaxle case and the adjustment shim installation surface using a depth gauge and straight edge.

2. Measure dimension O2 for the transaxle case installation surface of the clutch housing and the primary shaft rear bearing contact face using a depth gauge and straight edge.

  Note

  • Select only one adjustment shim.

3. Install the selected primary shaft rear bearing adjustment shim in the primary shaft component.