#
SLIDING DOOR STOPPER AND CONTROL LEVER REMOVAL/INSTALLATION

BME0911739A0203

1. Remove the left side trunk side trim.

2. Open the sliding door and remove the bolts of the sliding door stopper.

3. Close the sliding door.

4. Open the fuel-filler lid opener and remove the nut of the stopper control lever.

5. Disconnect the sliding door stopper cable from the fuel-filler lid opener.

6. Disconnect the rod.

7. Remove the sliding door stopper.

8. Remove the stopper control lever.

9. Install in the reverse order of removal.