#
CONTROL SYSTEM DEVICE AND CONTROL RELATIONSHIP CHART [AJ]

BME010300103201
×: Applicable

Component |  |  |  |  |  |  |  |  |  |  |  |  |
Input
Brake switch |  | × |  |  |  |  |  |  |  |  |  |  |
Refrigerant pressure switch, A/C switch, blower fan switch and A/C amplifier | × | × |  |  |  |  | × |  |  |  | × |  |
CKP sensor | × | × | × | × | × |  |  | × | × | × |  | × |
CMP sensor |  | × | × |  |  |  |  |  |  |  |  |  |
VSS |  | × | × |  |  |  |  |  | × |  |  | × |
EGR boost sensor (BARO sensor) |  | × | × |  |  |  |  | × |  |  |  |  |
MAF sensor | × | × | × |  | × |  |  | × | × |  |  |  |
ECT sensor | × | × | × |  | × | × | × | × | × | × | × | × |
IAT sensor | × | × |  |  |  |  |  | × | × |  |  | × |
TP sensor | × | × | × |  |  |  | × |  | × | × | × | × |
Front HO2S |  | × |  |  |  |  |  |  |  |  |  |  |
Knock sensor |  |  | × |  |  |  |  |  |  |  |  |  |
TR switch | × | × | × |  |  |  |  |  |  |  |  |  |
PSP switch | × | × | × |  |  |  |  |  |  |  | × |  |
Generator (terminal P: output voltage) | × |  |  |  |  |  |  |  |  |  |  | × |
DLC in engine compartment (TEN) | × |  | × |  |  |  | × |  |  |  |  |  |
Battery positive voltage |  | × | × |  |  |  |  | × |  |  |  | × |
Immobilizer unit |  | × | × |  |  |  |  |  |  |  |  |  | ×
Output
IAC valve | × |  |  |  |  |  |  |  |  |  |  |  |
Fuel injectors |  | × |  |  |  |  |  |  |  |  |  |  | ×
Ignition coil |  |  | × |  |  |  |  |  |  |  |  |  | ×
Fuel pump relay |  |  |  | × |  |  |  |  |  |  |  |  |
Front HO2S heater |  |  |  |  | × |  |  |  |  |  |  |  |
Rear HO2S heater* |  |  |  |  |  | × |  |  |  |  |  |  |
Fan control module |  |  |  |  |  |  | × |  |  |  |  |  |
Purge solenoid valve |  |  |  |  |  |  |  | × |  |  |  |  |
EGR valve |  |  |  |  |  |  |  |  | × |  |  |  |
IMCC actuator |  |  |  |  |  |  |  |  |  | × |  |  |
A/C relay |  |  |  |  |  |  |  |  |  |  | × |  |
Generator (terminal D: field coil) |  |  |  |  |  |  |  |  |  |  |  | × |
Generator warning light |  |  |  |  |  |  |  |  |  |  |  | × |

  * :
(European (L.H.D.) specs.)