#
REAR COMBINATION LIGHT REMOVAL/INSTALLATION

BME091851150W01

1. Disconnect the negative battery cable.

2. Remove the trunk side trim. (Right side only) (See TRUNK SIDE TRIM REMOVAL/INSTALLATION.)

3. Remove in the order indicated in the table.

1 | Connector
2 | Screw
3 | Rear combination light (See Rear Combination Light Removal Note)
4 | Socket (See Socket Installation Note)
5 | Brake light/taillight bulb
6 | Rear turn light bulb
7 | Back-up light bulb
8 | Rear fog light bulb (driver's side only)

4. Install in the reverse order of removal.

## Rear Combination Light Removal Note

1. Slide the rear combination light outward from the vehicle and disengage the attachment pins.

## Socket Installation Note

1. Hook the harness as shown in the figure.