#
DTC 11

BME010266350213

DTC 11 | Cruise control switch (SET/COAST switch)
--- | ---
DETECTION CONDITION | • Resistance detected between cruise actuator connector terminal J and ground is always approximately 198 ohms.
POSSIBLE CAUSE | • Cruise actuator malfunction • Cruise control switch malfunction

Diagnostic procedure

INSPECTION | ACTION
--- | ---
INSPECT DTC FOR OPERATION MODE • Was operation mode for DTC 21 performed? | Yes | Perform operation mode for DTC 21 on-board diagnostic again. Even if no malfunctions are detected in operation mode, if DTC 11 is indicated in condition detection mode on-board diagnostic, replace cruise actuator. (See CRUISE ACTUATOR REMOVAL/INSTALLATION)
No | Perform operation mode for DTC 21.