#
INSTRUMENT CLUSTER REMOVAL/INSTALLATION

BME092255430W01

1. Disconnect the negative battery cable.

2. Pull down the adjusting lever of the tilt steering wheel and push the steering wheel down.

3. Remove the meter hood.

4. Pull down the selector lever to the D range position.

5. Remove in the order indicated in the table.

6. Install in the reverse order of removal.

1 | Screw
2 | Connector
3 | Instrument cluster (See Instrument Cluster Removal Note.)

## Instrument Cluster Removal Note

1. When removing the instrument cluster, in order to prevent damage to the lens, cover the steering shaft with a cloth.