#
DTC 00 ERR03 OR 00:ER03

BME090266900W16

DTC 00 ERR03 or 00:Er03 | Cassette deck
DETECTION CONDITION | • Base unit detects that reel built into cassette deck does not operate.
POSSIBLE CAUSE | • Defective cassette tape (tape slack, pinched tape in internal cassette deck) • Cassette deck malfunction

Diagnostic procedure

STEP | INSPECTION | ACTION
--- | --- | ---
1 | INSPECT CASSETTE TAPE • Inspect condition of cassette tape where error has occurred. • Is cassette tape okay? | Yes | Go to next step.
No | Repair (remove tape slack or repair pinched tape) or replace cassette tape, then go to next step.
2 | INSPECT CASSETTE DECK • Clear DTC. • Insert cassette tape with no defect. • Play cassette tape for 20 seconds or more. • Start on-board diagnostic test mode.
• Is DTC 00 ERR03 or 00:Er03 displayed?
Yes
Replace cassette deck.
No | Troubleshooting completed.