#
IGNITION COIL INSPECTION [L3]

BME011818100W03

## Primary coil winding

1. Disconnect the ignition coil connector.

2. Measure the resistance between the following terminals using an ohmmeter:

  • A and B, B and C
  - If not within the specification, replace the ignition coil.

Resistance

  0.49-0.57 ohms

## Secondary Coil Winding

1. Disconnect the ignition coil connector.

2. Remove the ignition coil.

3. Measure the resistance between the following using an ohmmeter:

  • Lead hole 1 to 4, 2 to 3
  - If not within the specification, replace the ignition coil.

Resistance

  9.5-11.1 kilohms

## Insulation Resistance of Case

1. Disconnect the high-tension lead.

2. Disconnect the ignition coil connector.

3. Measure the insulation resistance from terminal B to ignition coil case using an ohmmeter.

  • If not within the specification, replace the ignition coil.

Resistance

  10 megohms or more