#
IGNITION COIL REMOVAL/INSTALLATION [L3]

BME011818100W01

  Caution

  • Disconnecting the ignition coil and plug cap can tear the plug cap off and cause damage to the connecting part. Disconnect the ignition coil and plug cap only when each component needs to be replaced, and be careful not to tear and damage them.

1. Disconnect the negative battery cable.

2. Remove in the order indicated in the table.

3. Install in the reverse order of removal.

1 | Connector
2 | High-tension lead (See HIGH-TENSION LEAD REMOVAL/INSTALLATION [L3].)
3 | Ignition coil