#
THEFT-DETERRENT RELAY REMOVAL/INSTALLATION

BME091450000201

  Note

  • Because the lock section of the relay is damaged easily, do not remove the relay from the bracket unless replacement is necessary. Always perform an inspection of the theft-deterrent relay before removal.

1. Disconnect the negative battery cable.

2. Remove the bracket.

3. Disconnect the theft-deterrent relay connector.

4. Remove the theft-deterrent relay by prying the lock section of the side part with a flathead screwdriver.

5. Install in the reverse order of removal.