#
FRONT DOOR ADJUSTMENT

BME091158010203

1. Measure the gap and height between the front door and the body.

2. If not as specified, loosen the door hinge installation bolts or the door lock striker installation screws, and reposition the door.

Clearance

  a: 4.0-6.0 mm {0.16-0.23 in}
  b: -1.0-1.0 mm {-0.03-0.03 in}
  c: 3.5-6.5 mm {0.14-0.25 in}
  d: -1.5-1.5 mm {-0.05-0.05 in}

3. Tighten the bolts or screws.