#
RANGE DETERMINATION OPERATION [FN4A-EL]

BME051718880T31
• Each range is determined by operating the selector lever, and switching on/off the switch in the TR switch internal circuit. The present range is detected according to the on/off signal of the switch.
• The following switches are built into the TR switch, and determine each range when the switch is on.
P and N position switch
R position switch
D range switch
S range switch
L range switch
• The range is determined to be R when there is no signal from the range switch, and a pre-programmed time has passed.