#
REAR WASHER NOZZLE REMOVAL/INSTALLATION

BME091967511201

1. Disconnect the negative battery cable.

2. Remove the liftgate lower trim.

3. Remove the rear washer hose from the rear washer nozzle.

4. Compress the tabs of the rear washer nozzle.

5. Pull the rear washer nozzle out to remove it.

6. Install in the reverse order of removal.

7. Adjust the rear washer nozzle. (See REAR WASHER NOZZLE ADJUSTMENT.)