#
FRONT AND REAR FOG LIGHT SWITCH, REAR FOG LIGHT SWITCH REMOVAL/INSTALLATION

BME091866402W01

1. Disconnect the negative battery cable.

2. Remove the driver-side side panel.

3. Remove in the order indicated in the table.

4. Install in the reverse order of removal.

1 | Front and rear fog light switch, Rear fog light switch (See Front and Rear Fog Light Switch, Rear Fog Light Switch Removal Note.)
2 | Connector

## Front and Rear Fog Light Switch, Rear Fog Light Switch Removal Note

1. Insert your hand into the hole for the driver-side side panel, squeeze the tabs of the front and rear fog light switch and pull it forward to remove it.