#
ENGINE COOLANT LEAKAGE INSPECTION

BME011215001206

1. Inspect the coolant level.

2. Remove the cooling system cap.

3. Connect a radiator cap tester and the SSTs to the reservoir filler port.

  Caution

  • Applying more than 123 kPa {1.25 kgf/cm2, 17.8 psi} can damage the hoses, fittings, and other components, and cause leaks.

4. Apply specified pressure to the radiator.

Pressure

  123 kPa {1.25 kgf/cm2, 17.8 psi}

5. Verify that the pressure is held.

  • If it exceeds the specification, inspect the system for coolant leakage.