#
NO.3 WILL NOT CRANK [MZR-CD (RF Turbo)]

BME010300000W38

3 | WILL NOT CRANK
--- | ---
DESCRIPTION | • Starter does not work.
POSSIBLE CAUSE | • Open starter circuit between engine switch and starter • Starter malfunction • Seized/hydrolocked engine, flywheel

Diagnostic procedure

STEP | INSPECTION | RESULTS | ACTION
--- | --- | --- | ---
1 | Inspect followings: • Battery connection • Battery condition • Fuses Are all items okay? | Yes | Go to next step.
No | Service as necessary. Repeat Step 1.
2 | Is clicking sound heard from starter when engine switch is turned to START? | Yes | Go to Step 4.
No | Go to next step.
3 | Inspect starting system. Is starting system okay? | Yes | Inspect for seized/hydrolocked engine, flywheel.
No | Repair or replace components as required.
4 | Do any other electrical accessories work? | Yes | Go to next step.
No | Inspect charging system.
5 | Connect WDS or equivalent to DLC-2. Turn engine switch to ON. Retrieve any DTC. Is DTC displayed? | Yes | DTC is displayed: Go to appropriate DTC test. Communication error message is displayed: Inspect for following: • Open circuit between PCM control relay and PCM terminal 53 or 79
• Open circuit PCM control relay and PCM terminal 69
• PCM control relay stuck open
• Open or poor GND circuit (PCM terminal 65, 85, 103 or 104)
• Poor connection vehicle body GND
No | No DTC is displayed: Inspect for following: • START circuit in engine switch • Open circuit between engine switch and starter
6 | Verify test results. • If okay, return to diagnostic index to service any additional symptoms. • If malfunction remains, replace PCM. (See PCM REMOVAL/INSTALLATION [MZR-CD (RF Turbo)].)