#
FRONT SEAT REMOVAL/INSTALLATION

BME091357100201

  Warning

  • Handling the front seat (side air bag) improperly can accidentally deploy the side air bag, which may seriously injure you. Read AIR BAG SYSTEM SERVICE WARNINGS before handling the front seat. (See SERVICE WARNINGS.)

1. Turn the ignition switch to the LOCK position.

2. Disconnect the negative battery cable and wait for more than 1 minute.

3. Remove in the order indicated in the table.

4. Install in the reverse order of removal.

1 | Side air bag module connector
2 | Buckle switch connector (Australian, General (L.H.D) specs.: driver's side only)
3 | Front seat