#
HYDRAULIC LASH ADJUSTER (HLA) REMOVAL/INSTALLATION [AJ]

BME011012100201

1. Disconnect the negative battery cable.

2. Remove the splash shield (RH).

3. Remove the dynamic chamber. (See INTAKE-AIR SYSTEM REMOVAL/INSTALLATION [AJ].)

4. Remove the drive belt.

5. Remove the ignition coils. (See IGNITION COIL REMOVAL/INSTALLATION [AJ].)

6. Remove the water pump drive belt. (See TIMING CHAIN REMOVAL/INSTALLATION [AJ].)

7. Remove the water pump drive belt pulley. (See Water Pump Drive Belt Pulley Removal Note.) (See Water Pump Drive Belt Pulley Installation Note.)

8. Remove the camshaft oil seal. (See Camshaft Oil Seal Removal Note.) (See Camshaft Oil Seal Installation Note.)

9. Remove the camshaft oil seal housing.

10. Remove in the order indicated in the table.

11. Install in the reverse order of removal.

1 | Engine hanger (LH) (See Engine Hanger Removal Note.) (See Engine Hanger Installation Note.)
2 | Oil level gauge pipe
3 | Cylinder head cover (LH) (See Cylinder Head Cover (LH) Removal Note.) (See Cylinder Head Cover (LH) Installation Note.)
4 | Condenser
5 | Engine hanger (RH) (See Engine Hanger Removal Note.) (See Engine Hanger Installation Note.)
6 | Cylinder head cover (RH) (See Cylinder Head Cover (RH) Removal Note.) (See Cylinder Head Cover (RH) Installation Note.)
7 | Crankshaft pulley lock bolt (See Crankshaft Pulley Lock Bolt Removal Note.) (See Crankshaft Pulley Lock Bolt Installation Note.)
8 | Crankshaft pulley (See Crankshaft Pulley Removal Note.) (See Crankshaft Pulley Installation Note.)
9 | Camshaft cap bolts (RH) (See Camshaft Caps (RH) Removal Note.) (See Camshaft Caps (RH) Installation Note.)
10 | Rocker arm (RH) (See Rocker Arm (RH) Removal Note.)
11 | HLA (RH)
12 | Camshaft cap bolts (LH) (See Camshaft Caps (LH) Removal Note.) (See Camshaft Caps (LH) Installation Note.)
13 | Rocker arm (LH) (See Rocker Arm (LH) Removal Note.)
14 | HLA (LH)

## Camshaft Caps (RH) Removal Note

1. Perform Step 1 and 2 in TIMING CHAIN REMOVAL/INSTALLATION, Timing Chain Component (RH) Removal Note. (See Timing Chain Component (RH) Removal Note.)

2. Perform the same procedures as TIMING CHAIN REMOVAL/INSTALLATION, Camshaft Caps (RH) Removal Note. (See Camshaft Caps (RH) Removal Note.)

## Rocker Arm (RH) Removal Note

  Note

  • If the rocker arm and HLA are to be reused, mark their positions to make sure they are assembled in the original location.
  • Take care not to let the rocker arm slip into the timing chain cover when removing the rocker arm from engine front.

1. Lift the camshaft slightly.

2. Remove the twelve rocker arms.

## Camshaft Caps (LH) Removal Note

1. Perform Step 1 in TIMING CHAIN REMOVAL/INSTALLATION, Timing Chain Component (LH) Removal Note. (See Timing Chain Component (LH) Removal Note.)

2. Perform the same procedures as TIMING CHAIN REMOVAL/INSTALLATION, Camshaft Caps (LH) Removal Note. (See Timing Chain Component (LH) Removal Note.)

## Rocker Arm (LH) Removal Note

  Note

  • If the rocker arm and HLA are to be reused, mark their positions to make sure they are assembled in the original location.
  • Take care not to let the rocker arm slip into the timing chain cover when removing the rocker arm from engine front.

1. Lift the camshaft slightly.

2. Remove the twelve rocker arms.

## Camshaft Caps (LH) Installation Note

1. Perform Steps 1, 2, 3 and 5 in TIMING CHAIN REMOVAL/INSTALLATION, Timing Chain Component (LH) Installation Note. (See Timing Chain Component (LH) Installation Note.)

## Camshaft Caps (RH) Installation Note

1. Perform Steps 1, 2, 3 and 5 in TIMING CHAIN REMOVAL/INSTALLATION, Timing Chain Component (RH) Installation Note. (See Timing Chain Component (RH) Installation Note.)