#
SLIDING DOOR LOCK ACTUATOR INSPECTION

BME091473380W02

## Door Lock Actuator

1. Remove the sliding door trim.

2. Partially peel off the door screen.

3. Disconnect the sliding door lock actuator connector.

4. Apply battery positive voltage to the sliding door lock actuator terminals and inspect the operation of the sliding door lock actuator.

  • If not as specified, replace the sliding door lock actuator.

Without double locking system

Connection | Actuator operation
--- | ---
B+ | GND
B | E | Lock
E | B | Unlock

With double locking system

Connection | Actuator operation
--- | ---
B+ | GND
E | B | Lock
E | C | Double lock
B and C | E | Unlock

## Door Lock-link Switch (With Theft-deterrent System)

  Note

  • The sliding door lock-link switch is together with the sliding door lock actuator.

1. Remove the sliding door trim.

2. Turn the door screen over.

3. Disconnect the sliding door lock actuator connector.

4. Inspect for continuity between the sliding door lock-link switch terminals using an ohmmeter.

  • If not as specified, replace the sliding door lock actuator.