#
REAR SHOCK ABSORBER DISPOSAL

BME021428700202

1. Clamp a shock absorber on a flat surface or with the piston pointing downwards.

2. Drill a 2-3 mm {0.08-0.12 in} hole at a point 20-30 mm {0.8-1.2 in} from the bottom of the tube, so that the gas can escape.

  Warning

  • The gas in the shock absorber is pressurized, and could spray metal chips into the eyes and face when drilling. Whenever drilling into a shock absorber, wear protective eye wear.

3. Turn the hole downwards.

4. Drain the oil by moving the piston rod several times up and down or cutting the tube at the end.

5. Dispose of waste oil according to the waste disposal law.

  Note

  • Shock absorber gas is nitrogen gas.
  • Shock absorber oil is mineral oil.