#
VANITY MIRROR ILLUMINATION BULB REMOVAL/INSTALLATION

BME091869270W01

1. Disconnect the negative battery cable.

2. Remove the sunvisor.

3. Insert a tape-wrapped flathead screwdriver into the service hole.

4. Twist the flathead screwdriver to remove the lens.

5. Unhook the hooks using a tape-wrapped flathead screwdriver.

6. Remove the mirror unit.

7. Remove the vanity mirror illumination bulbs.

8. Install in the reverse order of removal.