#
ENGINE CONTROL SYSTEM LOCATION INDEX [L3]

BME014000000W01

.

1 | PCM (See PCM REMOVAL/INSTALLATION [L3]) (See PCM INSPECTION [L3])
2 | MAF/IAT sensor (See MASS AIR FLOW (MAF) SENSOR INSPECTION [L3]) (See INTAKE AIR TEMPERATURE (IAT) SENSOR INSPECTION [L3])
3 | TP sensor (See THROTTLE POSITION (TP) SENSOR INSPECTION [L3])
4 | MAP sensor (See MANIFOLD ABSOLUTE PRESSURE (MAP) SENSOR INSPECTION [L3])
5 | ECT sensor (See ENGINE COOLANT TEMPERATURE (ECT) SENSOR REMOVAL/INSTALLATION [L3]) (See ENGINE COOLANT TEMPERATURE (ECT) SENSOR INSPECTION [L3])
6 | CMP sensor (See CAMSHAFT POSITION (CMP) SENSOR INSPECTION [L3])
7 | CKP sensor (See CRANKSHAFT POSITION (CKP) SENSOR INSPECTION [L3]) (See CRANKSHAFT POSITION (CKP) SENSOR REMOVAL/INSTALLATION [L3])
8 | Knock sensor (See KNOCK SENSOR INSPECTION [L3]) (See KNOCK SENSOR REMOVAL/INSTALLATION [L3])
9 | Front HO2S sensor (integrated O2S heater) (See HEATED OXYGEN SENSOR (HO2S) INSPECTION [L3])
10 | Rear HO2S sensor (integrated O2S heater) (See HEATED OXYGEN SENSOR (HO2S) INSPECTION [L3])
11 | BARO sensor (See BAROMETRIC PRESSURE (BARO) SENSOR INSPECTION [L3])
12 | Neutral switch (See NEUTRAL SWITCH INSPECTION [L3])
13 | Clutch switch (See CLUTCH SWITCH INSPECTION [L3])
14 | PSP switch (See POWER STEERING PRESSURE (PSP) SWITCH INSPECTION [L3])
15 | Main relay (See RELAY INSPECTION)