#
DRIVER-SIDE POWER WINDOW MOTOR RESETTING

BME091259560202

  Caution

  • The initial position of a new power window regulators has been preset. It is not necessary to reset the power window motor.
  • The initial position of a new power window motor has been preset. Begin from Step 3.
  • The automatic window return may not operate properly if the following is performed on the front door.

  - The power window motor is operated without the door glass properly installed.
  - The door glass is replaced.
  - The glass run channel is replaced.
  - The power window regulator is removed.

1. Remove the power window motor from the frame. (See FRONT POWER WINDOW REGULATOR DISASSEMBLY/ASSEMBLY.)

2. Connect battery positive voltage to terminal G and ground to terminal A, and operate the output axis of the motor in the upward direction 4 seconds or more (6 turns or more).

Terminal | Motor operation
--- | ---
A | G
GND | B+ | UP

3. Position the glass installation hole of the carrier plate 270-300 mm {10.6-11.8 in} (the range in which the glass can be installed) from the bottom of the frame.

4. Install the power window motor to the frame.

5. Install the power window regulator to the front door.

6. Install the front door glass to the power window regulator.

7. Connect the power window main switch connector.

8. Connect the negative battery cable.

9. Turn ignition switch to ON position.

10. Close the power window by operating the power window switch.

  • In the event that the automatic window return operates after the window fully closes by auto close, repeat Step 2.

  Caution

  • Automatic window return may not operate immediately after the power window motor is reset. In the event that auto window return is operated, be sure to perform Step 10.

11. Inspect the automatic window return function. (See AUTOMATIC WINDOW RETURN FUNCTION INSPECTION.)