#
SIMULATION TEST [AJ] (VIN: JMZ LW19J7*# 300001-, JM0 LW10J300 300001-301405, JM6 LW10J300 300001-, JM8 LW28J**# 300001-301513)

BME010200000T13
• The simulation test items for the fuel and emission control systems are as shown in the table below.

Simulation item table

×: Applied
-: Not applied

Simulation item | Applicable component | Operation | Test condition | PCM terminal
--- | --- | --- | --- | ---
IG ON | Idle
ACCS | A/C relay | ON or OFF | × | × | 69
ALTF | Generator field coil control duty value | OFF | - | × | 53
CHRGLP | Generator warning light | ON or OFF | × | × | 98
EGRCHK*3 | EGR boost sensor solenoid valve | ON or OFF | × | × | 47
EVAPCP | Purge solenoid valve | For purge solenoid valve: Actuated by any duty value (0-100%) | × | × | 18
FAN DUTY | Fan control module | Actuated by any duty value(0-100%) | × | × | 44
FP | Fuel pump relay | ON or OFF | × | × | 80*2, 104*1
FUELPW1 | Fuel injection duration | Actuated +50%- -50% fuel injection time | - | × | 73, 74, 75, 99, 100, 101
IAC | Idle air control valve | Actuated by any duty value(0-100%) | × | × | 54, 83
INJ#1 | Fuel injector (Cylinder No.1) | OFF | - | × | 75
INJ#2 | Fuel injector (Cylinder No.2) | OFF | - | × | 101
INJ#3 | Fuel injector (Cylinder No.3) | OFF | - | × | 74
INJ#4 | Fuel injector (Cylinder No.4) | OFF | - | × | 100
INJ#5 | Fuel injector (Cylinder No.5) | OFF | - | × | 73
INJ#6 | Fuel injector (Cylinder No.6) | OFF | - | × | 99
IVC | IMCC actuator | ON or OFF | × | × | 28
SEGRP | EGR valve (stepping motor) | Actuated by any stepping value (0-60 steps) | × | × | 12, 46, 56, 72

  *1 :
With immobilizer system
  *2 :
Without immobilizer system
  *3 :
Australian, General (L.H.D. R.H.D.) specs